|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | |  |  |  | |  |  |  | | | |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | |  |  | OFF | | 18° |  | 21° | | ***HAPCAN*** | | | |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | |  |  |  | |  |  |  | | ***HAPCAN*** | | |
| |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | |  |  |  | |  |  |  | |  | | | |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | | 15min |  |  | |  |  |  | |  | | |  |
| |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  |  | | --- | --- | --- | |  |  |  | |  |  |  | |  |  |  | | ***HAPCAN*** | | |  | Icons thanks to  http://icons8.com/ |
| **How to prepare touch panel labels**   1. Print required design on adhesive transparent foil and let it dry 2. Cut A4 page along the red line into single labels 3. Put another protective adhesive transparent foils on top of the printed ones 4. Cut the label to the required size along the light gray line 5. Stick the label on the Touch Panel and press it precisely 6. Cut temperature sensor hole using thin saw file with the sharp end | **Instrukcja wykonania etykiety panelu dotykowego**   1. Wydrukuj przygotowaną etykietę na samoprzylepnej przezroczystej folii i pozwól jej wyschnąć 2. Rozetnij stronę A4 wzdłuż czerwonej linii na pojedyncze etykiety 3. Przyklej jeszcze jedną ochronną wierzchnią warstwę samoprzylepnych folii na wydrukowane etykiety 4. Przytnij etykietę do wymaganego rozmiaru wzdłuż jasnoszarej linii 5. Przyklej etykietę na panel dotykowy i starannie dociśnij 6. Wytnij otwór sensora temperatury używając cienkiego okrągłego pilnika modelarskiego z ostrym końcem |  |

This template link: <https://github.com/hapcan/UNIV_3.1.2.x/blob/master/Touch_Panel/Touch_Panel_for_Gira55/touch_panel_gira_label.docx?raw=true>